ENABLED	XX

AUX 1

XX	ENABLED	XX

AUX 1

XX
TRIP
TRIP
INSTANTANEOUS	ENABLED

LOCK

DISABLED	INSTANTANEOUS	ENABLED

LOCK

DISABLED
PHASE OVRCURRENT
PHASE OVRCURRENT
GND/NEUTRAL OVERCURRENT	BLOCK CLOSE

CLOSE

BREAKER CLOSED	GND/NEUTRAL OVERCURRENT	BLOCK CLOSE

CLOSE

BREAKER CLOSED
NEG. SEQ. OVERCURRENT
NEG. SEQ. OVERCURRENT
OVER/UNDER FREQUENCY	XX

TRIP

BREAKER OPEN	OVER/UNDER FREQUENCY	XX

TRIP

BREAKER OPEN
BREAKER FAILURE
BREAKER FAILURE
ENABLED	XX

AUX 1

XX	ENABLED	XX

AUX 1

XX
TRIP
TRIP
INSTANTANEOUS	ENABLED

LOCK

DISABLED	INSTANTANEOUS	ENABLED

LOCK

DISABLED
PHASE OVRCURRENT
PHASE OVRCURRENT
GND/NEUTRAL OVERCURRENT	BLOCK CLOSE

CLOSE

BREAKER CLOSED	GND/NEUTRAL OVERCURRENT	BLOCK CLOSE

CLOSE

BREAKER CLOSED
NEG. SEQ. OVERCURRENT
NEG. SEQ. OVERCURRENT
OVER/UNDER FREQUENCY	XX

TRIP

BREAKER OPEN	OVER/UNDER FREQUENCY	XX

TRIP

BREAKER OPEN
BREAKER FAILURE
BREAKER FAILURE

Set printer to single, not duplex, printing.

Template for 198-0428

Tina L. Varey

2009-02-04

ericis

Schweitzer Engineering Laboratories, Inc.