Information gathered on a known good unit: 






N to L2  .0382Ω
       Transformer CT1 X1 to X2 1Ω

Exciter stator PM + to PM – 2.35Ω

Field amps 7

N to L1  .0387Ω



G1 to L1 .25Ω

F1 to F2 field  9.86Ω



Field volts 80
L1 to L2 .0734Ω



G1 to G2 .25Ω

Reactor X1 to X2 .8Ω calculated
