Most

TD1, TD3, LR1, AVR1, AVR3, KL1, AND KL3 

series PTO units CAN HAVE THE VOLTAGE REGULATOR REPLACED WITH A SE350 

(must be able to get 208 to 240 to the regulator) and unit must be brushless

NO 

EGO4, 150S, and 100s and 200s and250s PTO units CAN BE UPGRADED TO A SE350

